[SELECT_PARTS_DIALOG]
; 01000225
GUIDANCE="Select from the chart below the parts you replaced or remove and click the OK button. The required adjustments will automatically be decided and the correct order in which they are to be performed will be displayed."
GUIDANCE_dir="0"

[INDIVIDUAL_LIST]
; 01000161
GUIDANCE="Select an adjustment item from the below window and double-click to execute it."
GUIDANCE_dir="0"

[EEPROM_COPY]
; 01000246
GUIDANCE="This function copies selected data from current main board to new main board.\r\n1) Please select item that dose backup.\r\n2) Click [Backup] button to backup selected data from current main board.\r\n3) Turn off the printer and replace current main board with new one.\r\n4) Turn on the printer again and click [Restore] button to save selected data on new main board."
GUIDANCE_dir="0"

[EEPROM_INITIALIZE]
; 01000130
GUIDANCE="NOTE : Please don't execute this function when backing up the EEPROM data with EEPROM Data Copy function.\r\n\r\n1) Please select item that does initialization, and click the [Perform] button.\r\n    -[Initial setting] : Writing initial setting value to EEPROM.\r\n    -[Product Serial No.] : Writing Product Serial No. to EEPROM.\r\n    -[MAC Address] : Writing MAC Address to EEPROM.\r\n    -[Mechanism No.] : Writing specific control data to EEPROM. (EURO Only)\r\n2) Click the [Check] button to read out current setting values."
GUIDANCE_dir="0"

[PF_DETERIORATION_OFFSET]
; 01000207
GUIDANCE="1) Click [Initialization] button to reset current PF deterioration value to \"Zero\"."
GUIDANCE_dir="0"

[PWSENSOR_DETERIORATION_COUNTER_INIT]
; 01000273
GUIDANCE="1) Click [Initialization] button to reset current PW sensor deterioration counter to \"Zero\"."
GUIDANCE_dir="0"

[HEAD_ID_INPUT]
; 01000155
GUIDANCE="[Method to input the Head ID]\r\n1) Input Head ID in the edit box.\r\n2) Click [Input] button to record Head ID to the EEPROM.\r\n     If error message is displayed, please input Head ID again.\r\n\r\n[How to check current Head ID]\r\n1) Click [Check] button to check current Head ID."
GUIDANCE_dir="0"

[HEAD_ID_AUTO_INPUT]
GUIDANCE="1) Click [Auto Input] button to record Head ID automatically. If the print head was replaced, must be input Head ID.\r\n2) Click [Verify] button to verify current Head ID is correctly."
GUIDANCE_dir="0"

[HEAD_ANGULAR_MECHA]
GUIDANCE="1) Print Adjustment Pattern\r\n   Set A4 size Matte paper in the Cassette 1, then click the [Print] button.\r\n2) Adjustment\r\n  According to print pattern, adjust head angular by using the head adjustment lever."
GUIDANCE_dir="0"

[HEAD_ANGULAR]
; 01000257
GUIDANCE="1) Set A4 size Plain Paper in the Cassette 1.\r\n2) Click [Print] button to print a check pattern.\r\n3) Choose the number of the pattern having the best alignment from the printed check pattern.\r\n4) Input the number in the edit box (both "1 to 80" and "80 to 1" side).\r\n5) Click [Input] button to record the correction parameter to the EEPROM."
GUIDANCE_dir="0"

[PF_ADJUSTMENT]
; 01000198
GUIDANCE="1) Set A4 size Matte Paper in the Cassette 1.\r\n2) Click [Print] button to print check pattern.\r\n3) Select the number of the pattern with the best alignment from the list.\r\n4) Choose the selected pattern from the edit box.\r\n5) Click [Input] button to record the parameter to the EEPROM."
GUIDANCE_dir="0"

[PW_ADJUSTMENT]
; 01000274
GUIDANCE="1) Set A4 size Matte Paper in the Cassette 1 and A4 size Plain Paper in the Cassette 2.\r\n2) Click [Print] button to print check pattern.\r\n3) Select the number of the pattern with the best alignment from the list.\r\n4) Choose the selected pattern from the edit box.\r\n5) Click [Input] button to record the parameter to the EEPROM.\r\n\r\n[How to select the best line]\r\n1) The printed line on should be 5mm away from each of the paper's edges.\r\n2) Choose the selected pattern from edit box."
GUIDANCE_dir="0"

[PE_ADJUSTMENT]
; 01000268
GUIDANCE="1) Set A4 size Plain Paper in the Cassette 1.\r\n2) Click [Perform] button to perform PE adjustment and record the adjustment value to the EEPROM."
GUIDANCE_dir="0"

[PTS_DELAY_ADJUSTMENT]
GUIDANCE="1) Set A4 size Plain Paper in the Cassette 1.\r\n2) Click [Print] button to print PTS check pattern.\r\n3) Select the number of the pattern with the best alignment and input the edit box.\r\n4) Click [Input] button to record the parameter to the EEPROM.\r\n"
GUIDANCE_dir="0"

[MANUAL_BID]
; 01000258
GUIDANCE="1) Set A4 size Plain Paper in the Cassette 1.\r\n2) Click [Print] button to print check pattern of selected dot size.\r\n3) Select the number of the pattern with the best alignment from the list.\r\n4) Choose the selected pattern from the edit box.\r\n5) Click [Input] button to record the parameter to the EEPROM.\r\n    For the case where there is no best pattern, you should input the maximum or\r\n     minimum parameter of the test pattern which ever is most appropriate.\r\n     The offset value will be printed in the center position the next time the check pattern is printed.\r\n     Please repeat this adjustment until you can select the best pattern."
GUIDANCE_dir="0"

[PF_BAND_ADJUSTMENT]
; 01000275
GUIDANCE="1) Set A4 size Plain Paper in the Cassette 1.\r\n2) Click [Print] button to print check pattern.\r\n3) Select the number of the pattern with the best alignment from the list.\r\n4) Choose the selected pattern from the edit box.\r\n5) Click [Input] button to record the parameter to the EEPROM."
GUIDANCE_dir="0"

[PS_ADJUSTMENT]
; 01000276
GUIDANCE="NOTE : Adjust Paper Skew after adjusting Bi-D.\r\n1) Set A4 size Plain Paper in the Cassette 1.\r\n2) Click [Print] button to print adjustment pattern.\r\n3) Select the value with the smallest gap respectively of Upper, Lower, and input it to the Edit box.\r\n4) Click [Input] button to save the adjustment value into EEPROM.\r\n5) Click the [Check] button to check the current adjustment values."
GUIDANCE_dir="0"

[HEAT_PROTECTION]
; 01000158
GUIDANCE="1) Select replacement parts from the following check boxes.\r\n2) Click [Perform] button to record the proper value of motor heat protection to the EEPROM for the selected replacement parts."
GUIDANCE_dir="0"

[PF_HEAT_PROTECTION]
; 01000211
GUIDANCE="1) Select replacement parts from the following check boxes.\r\n2) Click [Perform] button to record the proper value of PF motor heat protection to the EEPROM for the selected replacement parts."
GUIDANCE_dir="0"

[IS_HEAT_PROTECTION]
GUIDANCE="1) Select replacement parts from the following check boxes.\r\n2) Click [Perform] button to record the proper value of I/S motor heat protection to the EEPROM for the selected replacement parts."
GUIDANCE_dir="0"

[ASF_HEAT_PROTECTION]
; 01000277
GUIDANCE="1) Select replacement parts from the following check boxes.\r\n2) Click [Perform] button to record the proper value of ASF motor heat protection to the EEPROM for the selected replacement parts."
GUIDANCE_dir="0"

[SCN_HEAT_PROTECTION]
; 01000265
GUIDANCE="1) Select replacement parts from the following check boxes.\r\n2) Click [Perform] button to record the proper value of SCANNER/ADF motor heat protection to the EEPROM for the selected replacement parts."
GUIDANCE_dir="0"

[PE_DETECTOR_COMFIRM]
; 01000278
GUIDANCE="1) Set A4 size Plain Paper in the Cassette 1.\r\n2) Click [Perform] button, then the printer feeds the paper and check the PE detector sensor.\r\n3) If the result is NG, put together the lever of PE detector sensor again."
GUIDANCE_dir="0"

[CLEANING]
; 01000120
GUIDANCE="1) Click [Print] button to print nozzle check pattern print.\r\n2) If dot missing appears, click [Cleaning] button to perform a cleaning.\r\n3) Click [Print] button to print nozzle check pattern print again.\r\n4) If dot missing is not recovered, repeat from step 2) to step 3)"
GUIDANCE_dir="0"

[INK_CHARGE]
; 01000163
GUIDANCE="1) Click [Ink Charge] button to perform ink charge.\r\n2) Click [Print] button to print nozzle check pattern print.\r\n3) If dot missing appears, click [Cleaning] button to perform a cleaning.\r\n4) Click [Print] button to print nozzle check pattern print again.\r\n5) If dot missing is not recovered, repeat from step 3) to step 4)"
GUIDANCE_dir="0"

[INK_PAD_COUNTER]
; 01000171
GUIDANCE="1) Click [Check] button to check current counter's value.\r\n2) Click [Initialization] to reset selected counter to the initial value.\r\nNOTE: You have to initialize the counter if you replaced appropriate part with new one."
GUIDANCE_dir="0"

[SHIPPING_SETTING]
; 01000229
GUIDANCE="1) Click [Write] button to write the shipping setting.\r\n- If \"Cleaning flag set\" is checked, cleaning is executed at the next power ON. (Please use this function in case of nozzle clogging during transport.)" 
GUIDANCE_dir="0"

[CHECK_PATTERN_PRINT]
; 01000119
GUIDANCE="1) Set paper for selected pattern.\r\n2) Click [Print] button to print selected pattern."
GUIDANCE_dir="0"

[CHECK_PATTERN_PRINT_LS]
GUIDANCE="[Check Pattern Print]\r\n1) Click [Print] button to print selected pattern.\r\n\r\n[Limit Sample / Standard View]\r\n1) Click the [View] or [Standard] button to display the limit samples or standard corresponding to the item that is selected in the [Print]."
GUIDANCE_dir="0"

[EEPROM_READOUT]
; 01000133
GUIDANCE="1) Click [Dump] button to read out and save all of EEPROM data."
GUIDANCE_dir="0"

[OPERATION_INFO]
; 01000187
GUIDANCE="1) Click the [Check] button to read out the printer information.\r\n2) Click the [Error Detail] button to display error information."
GUIDANCE_dir="0"

[PAPER_FEED_TEST]
; 01000190
GUIDANCE="1) Set A4 size Plain Paper in the selected Cassette.\r\n2) Set the number of sheets and click [Perform] button."
GUIDANCE_dir="0"

[INK_FLUSHING]
GUIDANCE="Discharge the ink from Ink supply path by the following procedure when removing \r\nthe ink tube from print head.\r\n1) Open the ink case cover, and making the ink case cover open sensor closing \r\n  condition by tape.\r\n2) Remove the ink pack from ink case.\r\n3) Click the [Perform] then staring the ink discharge."
GUIDANCE_dir="0"

[INK_DISCHARGE]
; 01000267
GUIDANCE="1) Set the ink discharge jig and use shipping liquid.\r\n2) Chlick the [Perform] buttonto start the discharge.\r\n3) Afterexecute Ink discharge, click the [Perform] button to exectue shipping liquid discharge to prevent leak the shipping liquid outside the print head."
GUIDANCE_dir="0"

[FACTORY_SETTING]
GUIDANCE="1) After clicking the \"Write\" button, all the user settings will be cleared and the factory settings will be written to the devise.\r\n2) The factory settings will be recorded when the printer is turned off and applied automatically the next turned on.\r\n3) This function also have a initial charging and cleaning process performed automatically the next turned on."
GUIDANCE_dir="0"

[PIS_CHECK]
; 01000254
GUIDANCE="1) Click [Perform] button to check the PIS(Photo Ink Sensor) board.\r\n2) If the sensor has reached the end of its life, please replace the PIS board."
GUIDANCE_dir="0"

[CR_UNLOCK]
GUIDANCE="1) Click [Perform] button and turn the printer power OFF.\r\n CR is unlocked during the power OFF.\r\n This function is effective only one time."
GUIDANCE_dir="0"

[APG_OFFSET_ADJUSTMENT]
GUIDANCE="1) Click [Perform] button to adjust the APG offset."
GUIDANCE_dir="0"

[TOUCH_PANEL_CHECK]
GUIDANCE="1) Click [Perform] button to check the touch panel."
GUIDANCE_dir="0"

[TEMP_HUM_CHECK]
GUIDANCE="Check that the temperature and humidity sensors are operating normally.\r\n1) Click [Perform] button, and displaying the current temperature and Humidity."
GUIDANCE_dir="0"

[NVT_ADJUSTMENT]
GUIDANCE="Set the rank for setting the optimal judgment threshold value of each nozzle to ensure Nozzle diagnostic function detection accuracy.\r\n1) Click [Perform] button, and performing the Nozzle Rank Categorise. \r\n-Make sure to peform Nozzle Rank Categorise with all nozzle normally condition.\r\nIf "Error" is displayed, perform head cleaning to enable the state where all nozzles discharge ink normally\r\n2) Click [Check] button, and performing the nozzle detect check."
GUIDANCE_dir="0"

[NVT_LOG_TRACE]
GUIDANCE="Write the nozzle detect history to memory of the failure print head before replace the print head. \r\n-Make sure to perform this function before replacing the print head. \r\n  Because nozzle detect history is necessary to analyzing the failure print head.\r\n1) Click [Perform] button, and writing the nozzle detect history."
GUIDANCE_dir="0"