[SCN_100001]
MEANING="ADF PID excess speed error"
DESCRIPTION=" - Failed to read the ADF motor encoder\r\n   1. Contamination of the ADF encoder scale\r\n   2. Damage or skew of the ADF encoder FFC\r\n   3. Failure of the ADF encoder sensor\r\n - Failure of the ADF motor driver\r\n   4. Failure of the main board"

[SCN_100002]
MEANING="ADF PID reverse error"
DESCRIPTION=" - Paper feed fails, stopped by obstacles\r\n   1. Paper feed was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the paper feed mechanism\r\n      - Disengaging or tooth breakage of wheel train\r\n        of the paper feed mechanism\r\n - Failed to read the PF motor encoder\r\n   2. Jumping of the ADF timing belt\r\n   3. Contamination of the ADF encoder scale\r\n   4. Damage or skew of the ADF encoder FFC\r\n   5. Failure of the ADF encoder sensor\r\n   6. Failure of the main board"

[SCN_100003]
MEANING="ADF PID lock error"
DESCRIPTION=" - The ADF motor did not run or obstacles exist in the paper path\r\n1. Overload of the paper feed mechanism\r\n2. The ADF timing belt become frayed, jumping,\r\n    or the wheel train of paper feed mechanism\r\n    is disengaged or its tooth is broken\r\n - Failed to read the ADF motor encoder\r\n   3. Contamination of the ADF encoder scale\r\n   4. Disconnection, break, skew or damage of the ADF encoder FFC\r\n   5. Failure of the ADF encoder sensor\r\n   6. Failure of the ADF motor (the lead wire\r\n       is broken or the connector is disconnected)\r\n   7. Failure of the main board"

[SCN_100004]
MEANING="ADF PID acceleration lock error"
DESCRIPTION=""

[SCN_100005]
MEANING="ADF PID excess load error"
DESCRIPTION=" - The ADF motor stopped running in the middle of the operation\r\n   1. The ADF was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the paper feed mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the ADF motor encoder\r\n   2. The timing belt become frayed or jumping\r\n   3. Contamination of the ADF encoder scale\r\n   4. Disconnection, break, skew or damage\r\n       of the ADF motor cable/encoder FFC\r\n   5. Failure of the ADF motor (not completely broken)\r\n   6. Failure of the main board"

[SCN_100006]
MEANING="ADF PID driving time error"
DESCRIPTION="Malfunction or crash of the firmware"

[SCN_100009]
MEANING="ADF BS+ excess speed error"
DESCRIPTION=" - Failed to read the ADF motor encoder\r\n   1. Contamination of the ADF encoder scale\r\n   2. Damage or skew of the ADF encoder FFC\r\n   3. Failure of the ADF encoder sensor\r\n - Failure of the ADF motor driver\r\n   4. Failure of the main board"

[SCN_100010]
MEANING="ADF BS+ reverse error"
DESCRIPTION=" - Paper feed fails, stopped by obstacles\r\n   1. Paper feed was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the paper feed mechanism\r\n      - Disengaging or tooth breakage of wheel train\r\n        of the paper feed mechanism\r\n - Failed to read the ADF motor encoder\r\n   2. Jumping of the ADF timing belt\r\n   3. Contamination of the ADF encoder scale\r\n   4. Damage or skew of the ADF encoder FFC\r\n   5. Failure of the ADF encoder sensor\r\n   6. Failure of the main board"

[SCN_100011]
MEANING="ADF BS+ lock error"
DESCRIPTION=" - The ADF motor did not run\r\n   1. The ADF was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the ADF encoder\r\n   2. Contamination of the ADF encoder scale\r\n   3. Disconnection, break, skew or damage\r\n       of the ADF motor cable/encoder FFC\r\n   4. Failure of the ADF encoder sensor\r\n   5. Failure of the ADF motor (the lead wire is broken\r\n       or the connector is disconnected)\r\n   6. Failure of the main board"

[SCN_100013]
MEANING="ADF BS+ excess load error"
DESCRIPTION=" - The ADF motor stopped running in the middle of the operation\r\n   1. The ADF was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the paper feed mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the ADF motor encoder\r\n   2. Jumping of the timing belt\r\n   3. Contamination of the ADF encoder scale\r\n   4. Failure of the ADF motor (not completely broken)\r\n   5. Failure of the main board"

[SCN_100014]
MEANING="ADF BS+ driving time error"
DESCRIPTION="Malfunction or crash of the firmware"

[SCN_100016]
MEANING="HP detection failure"
DESCRIPTION=" - The scanner CR could not return to its home.\r\n   1. Damage or disengaging of wheel train of the drive mechanism\r\n   2. Disengaging, fraying, jumping of the timing belt\r\n - Failed to read the white standard/home patterns\r\n   3. Disconnection, break, skew or damage of the scanner FFC\r\n   4. Failure of the CIS unit\r\n   5. Failure of the scanner housing\r\n   6. Failure of the main board"

[SCN_100017]
MEANING="Contact detection distance exceeded"
DESCRIPTION=" - The scanner CR cannot completely reach the home (left side)\r\n   1. Damage or disengaging of wheel train of the drive mechanism\r\n - Failed to read the scanner encoder\r\n   2. Damage or skew of the scanner FFC\r\n   3. Failure of the CIS unit\r\n   4. Failure of the scanner housing\r\n   5. Failure of the main board"

[SCN_100018]
MEANING="Opposite side contact detection distance
exceeded error"
DESCRIPTION=" - The scanner CR cannot completely reach the opposite side of the home (right side)\r\n   1. Damage or disengaging of wheel train of the drive mechanism\r\n - Failed to read the scanner encoder\r\n   2. Damage or skew of the scanner FFC\r\n   3. Failure of the CIS unit\r\n   4. Failure of the scanner housing\r\n   5. Failure of the main board"

[SCN_100019]
MEANING="Wrong contact detection distance error"
DESCRIPTION="1. CIS Unit failure\r\n2. Scanner Housing failure (Including wrong attachment of the origin mark)\r\n3. Main Board failure\r\n4. Scanner FFC failure / Scanner FFC connection failure\r\n5. Scanner Motor failure / Scanner Motor connection failure"

[SCN_100020]
MEANING="Measurement error"
DESCRIPTION=" - Overload of the scanner drive mechanism\r\n - Failure of the scanner motor"

[SCN_100032]
MEANING="LED light failure"
DESCRIPTION=" - Failure of the CIS LED light (RGB)\r\n1. Disconnection, break, skew or damage of the scanner FFC\r\n2. Failure of the CIS unit\r\n3. Failure of the main board"

[SCN_100048]
MEANING="Option error"
DESCRIPTION="使用していない"

[SCN_100054]
MEANING="Paper jam error"
DESCRIPTION=" - No jammed paper is remaining but the sensor does not turn off\r\n   1. Failure of the ADF PE sensor\r\n   2. Failure of the cable\r\n - Jammed paper is remaining\r\n - The paper feed rollers and paper conveying rollers slip too much\r\n    -At power -on, during paper feed, during scanning"

[SCN_100065]
MEANING="FB PID excess speed error"
DESCRIPTION=" - Failed to read the scanner encoder\r\n   1. Contamination of the scanner encoder scale\r\n   2. Damage or skew of the scanner FFC\r\n   3. Failure of the scanner encoder sensor\r\n - Failure of the scanner motor driver\r\n   4. Failure of the main board"

[SCN_100066]
MEANING="FB PID reverse error"
DESCRIPTION=" - Operation failure of the scanner motor\r\n   1. The scanning operation was stopped by;\r\n      - Disengaging of the scanner CR\r\n      - Disengaging of the scanner motor pulley\r\n        or cracking of the scanner motor gears\r\n - Failed to read the scanner encoder\r\n   2. Contamination of the scanner encoder\r\n   3. Damage or skew of the scanner FFC\r\n   4. Failure of the scanner encoder sensor\r\n   5. Failure of the main board"

[SCN_100067]
MEANING="FB PID lock error"
DESCRIPTION=" - The scanner motor did not run\r\n   1. The scanning operation was stopped by;\r\n      - Disengaging of the scanner CR\r\n      - Disengaging of the scanner motor pulley\r\n        or cracking of the scanner motor gears\r\n - Failed to read the CR motor encoder\r\n   2. Contamination of the scanner encoder\r\n   3. Damage or skew of the scanner FFC\r\n   4. Failure of the scanner encoder sensor\r\n   5. Failure of the scanner motor\r\n   6. Failure of the main board"

[SCN_100068]
MEANING="FB PID acceleration lock error"
DESCRIPTION=" - The scanner motor did not run\r\n   1. The scanning operation was stopped by;\r\n      - Disengaging of the scanner CR\r\n      - Disengaging of the scanner motor pulley\r\n        or cracking of the scanner motor gears\r\n - Failed to read the scanner motor encoder\r\n   2. Contamination of the scanner encoder\r\n   3. Damage or skew of the scanner FFC\r\n   4. Failure of the scanner encoder sensor\r\n   5. Failure of the scanner motor"

[SCN_100069]
MEANING="FB PID excess load error"
DESCRIPTION=" - The scanner motor stopped running in the middle of the operation\r\n   1. The scanning operation was stopped by;\r\n      - Disengaging of the scanner CR\r\n      - Disengaging of the scanner motor pulley\r\n        or cracking of the scanner motor gears\r\n - Failed to read the scanner motor encoder\r\n   2. Contamination of the scanner encoder\r\n   3. Disconnection, break, skew or damage of the scanner FFC\r\n   4. Failure of the scanner encoder sensor\r\n   5. Failure of the scanner motor"

[SCN_100070]
MEANING="FB PID driving time error"
DESCRIPTION="Malfunction or crash of the firmware"

[SCN_100073]
MEANING="FB BS+ excess speed error"
DESCRIPTION=" - Failed to read the scanner encoder\r\n   1. Contamination of the scanner encoder scale\r\n   2. Damage or skew of the scanner FFC\r\n   3. Failure of the scanner encoder sensor\r\n - Failure of the scanner motor driver\r\n   4. Failure of the main board"

[SCN_100074]
MEANING="FB BS+ reverse error"
DESCRIPTION=" - Operation failure of the scanner motor\r\n   1. The scanning operation was stopped by;\r\n      - Disengaging of the scanner CR\r\n      - Disengaging of the scanner motor pulley\r\n        or cracking of the scanner motor gears\r\n - Failed to read the scanner encoder\r\n   2. Contamination of the scanner encoder\r\n   3. Damage or skew of the scanner FFC\r\n   4. Failure of the scanner encoder sensor\r\n   5. Failure of the main board"

[SCN_100075]
MEANING="FB BS+ lock error"
DESCRIPTION=" - The scanner motor did not run\r\n   1. The scanning operation was stopped by;\r\n      - Disengaging of the scanner CR\r\n      - Disengaging of the scanner motor pulley\r\n        or cracking of the scanner motor gears\r\n - Failed to read the CR motor encoder\r\n   2. Contamination of the scanner encoder\r\n   3. Damage or skew of the scanner FFC\r\n   4. Failure of the scanner encoder sensor\r\n   5. Failure of the scanner motor\r\n   6. Failure of the main board"

[SCN_100077]
MEANING="FB BS+ excess load error"
DESCRIPTION=" - The scanner motor stopped running in the middle of the operation\r\n   1. The scanning operation was stopped by;\r\n      - Disengaging of the scanner CR\r\n      - Disengaging of the scanner motor pulley\r\n        or cracking of the scanner motor gears\r\n - Failed to read the scanner motor encoder\r\n   2. Contamination of the scanner encoder\r\n   3. Disconnection, break, skew or damage of the scanner FFC\r\n   4. Failure of the scanner encoder sensor\r\n   5. Failure of the scanner motor\r\n   6. Failure of the main board"

[SCN_100078]
MEANING="FB BS+ driving time error"
DESCRIPTION="Malfunction or crash of the firmware"

[PRN_000020]
MEANING="CR PID driving time error"
DESCRIPTION="Malfunction or crash of the firmware"

[PRN_000021]
MEANING="CR PID excess load error"
DESCRIPTION=" - The CR motor stopped running in the middle of the operation\r\n   1. The CR was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the mechanism\r\n      - Interfere with the ink system\r\n      - Disengaging, fraying, jumping of the timing belt\r\n      - Crack or disengaging of the gear, or the APG\r\n       lever interferes with the CR\r\n - Failed to read the CR encoder\r\n   2. Contamination of the CR encoder scale\r\n   3. Failure of the CR motor (not completely broken)\r\n   4. Failure of the main board"

[PRN_000022]
MEANING="CR PID excess speed error"
DESCRIPTION=" - Failed to read the CR encoder\r\n   1. Contamination of the CR encoder scale\r\n   2. Damage or skew of the CR encoder FFC\r\n   3. Failure of the CR encoder sensor\r\n - Failure of the CR motor driver\r\n   4. Failure of the main board"

[PRN_000023]
MEANING="CR PID reverse error"
DESCRIPTION=" - Operation failure of the CR motor, stopped by obstacles\r\n   1. CR was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Interfere with the ink system\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the CR encoder\r\n   2. Jumping of the CR timing belt\r\n   3. Contamination of the CR encoder scale\r\n   4. Damage or skew of the CR encoder FFC\r\n   5. Failure of the CR encoder sensor\r\n   6. Failure of the main board"

[PRN_000024]
MEANING="CR PID lock error"
DESCRIPTION=" - The CR motor did not run, or the CR could not move smoothly\r\n   1. Overload of the CR\r\n - Failed to read the CR encoder\r\n   2. The timing belt become frayed or jumping\r\n   3. Contamination of the CR encoder scale\r\n   4. Disconnection, break, skew or damage of the CR encoder FFC\r\n   5. Failure of the CR encoder sensor\r\n   6. Failure of the CR motor (the lead wire is broken\r\n       or the connector is disconnected)\r\n   7. Failure of the main board"

[PRN_000025]
MEANING="CR PID speed fall error"
DESCRIPTION=" - Operation failure of the CR\r\n   1. The CR was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the mechanism\r\n      - Interfere with the ink system\r\n - Failed to read the CR motor encoder\r\n   2. The timing belt become loosened or jumping\r\n   3. Contamination of the CR encoder scale\r\n   4. Damage or skew of the CR encoder FFC\r\n   5. Failure of the CR motor\r\n   6. Failure of the main board"

[PRN_000030]
MEANING="CR load position driving time error"
DESCRIPTION="Malfunction or crash of the firmware"

[PRN_000031]
MEANING="CR load position excess load errorエラー"
DESCRIPTION=" - The CR motor stopped running in the middle of the operation\r\n   1. The CR was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the mechanism\r\n      - Interfere with the ink system\r\n      - Disengaging or breakage of the gears\r\n      - Disengaging, fraying, jumping of the timing belt\r\n - Failed to read the CR encoder\r\n   2. Contamination of the CR encoder scale\r\n   3. Failure of the CR motor (not completely broken)\r\n   4. Failure of the main board"

[PRN_000032]
MEANING="CR load position excess speed error"
DESCRIPTION=" - Failed to read the CR encoder\r\n   1. Contamination of the CR encoder scale\r\n   2. Damage or skew of the CR encoder FFC\r\n   3. Failure of the CR encoder sensor\r\n - Failure of the CR motor driver\r\n   4. Failure of the main board"

[PRN_000033]
MEANING="CR load position reverse error"
DESCRIPTION=" - Operation failure of the CR motor, stopped by obstacles\r\n   1. CR was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the mechanism\r\n      - Interfere with the ink system\r\n - Failed to read the CR encoder\r\n   2. Jumping of the CR timing belt\r\n   3. Contamination of the CR encoder scale\r\n   4. Damage or skew of the CR encoder FFC\r\n   5. Failure of the CR encoder sensor\r\n   6. Failure of the main board"

[PRN_000040]
MEANING="PF PID driving time error"
DESCRIPTION="Malfunction or crash of the firmware\r\n    -The PE sensor remains in paper detection status\r\n       and a paper jam error occurs instead of causing a fatal error."

[PRN_000041]
MEANING="PF PID excess load error"
DESCRIPTION=" - The PF motor stopped running in the middle of the operation\r\n   1. The PF was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the paper feed mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the PF motor encoder\r\n   2. The timing belt become frayed or jumping\r\n   3. Contamination of the PF encoder scale\r\n   4. Disconnection, break, skew or damage\r\n       of the PF motor cable/encoder FFC\r\n   5. Failure of the PF motor (not completely broken)\r\n   6. Failure of the main board"

[PRN_000042]
MEANING="PF PID excess speed error"
DESCRIPTION=" - Failed to read the PF motor encoder\r\n   1. Contamination of the PF encoder scale\r\n   2. Skew or damage of the PF encoder FFC\r\n   3. Failure of the PF encoder sensor\r\n - Failure of the PF motor driver\r\n   4. Failure of the main board"

[PRN_000043]
MEANING="PF PID reverse error"
DESCRIPTION=" - Paper feed fails, stopped by obstacles\r\n   1. Paper feed was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the paper feed mechanism\r\n      - Disengaging or tooth breakage of wheel train\r\n        of the paper feed mechanism\r\n - Failed to read the PF motor encoder\r\n   2. Jumping of the PF timing belt\r\n   3. Contamination of the PF encoder scale\r\n   4. Skew or damage of the PF encoder FFC\r\n   5. Failure of the PF encoder sensor\r\n   6. Failure of the main board"

[PRN_000044]
MEANING="PF PID lock error"
DESCRIPTION=" - The PF motor did not run or obstacles exist in the paper path\r\n   1. Overload of the paper feed mechanism\r\n   2. The PF timing belt become frayed, jumping,\r\n        or the wheel train of paper feed mechanism\r\n        is disengaged or its tooth is broken\r\n - Failed to read the PF motor encoder\r\n   3. Contamination of the PF encoder scale\r\n   4. Disconnection, break, skew or damage of the PF encoder FFC\r\n   5. Failure of the PF encoder sensor\r\n   6. Failure of the PF motor (the lead wire is broken\r\n       or the connector is disconnected)\r\n   7. Failure of the main board"

[PRN_000050]
MEANING="PF load position driving time error"
DESCRIPTION="Malfunction or crash of the firmware"

[PRN_000051]
MEANING="PF load position excess load error"
DESCRIPTION=" - The PF motor stopped running in the middle of the operation\r\n   1. The PF was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the paper feed mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the PF motor encoder\r\n   2. Jumping of the timing belt\r\n   3. Contamination of the PF encoder scale\r\n   4. Failure of the PF motor (not completely broken)\r\n   5. Failure of the main board"

[PRN_000052]
MEANING="PF load position excess speed error"
DESCRIPTION=" - Failed to read the PF motor encoder\r\n   1. Contamination of the PF encoder scale\r\n   2. Skew or damage of the PF encoder FFC\r\n   3. Failure of the PF encoder sensor\r\n - Failure of the PF motor driver\r\n   4. Failure of the main board"

[PRN_000053]
MEANING="PF load position reverse error"
DESCRIPTION=" - Paper feed fails, stopped by obstacles\r\n   1. Paper feed was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the paper feed mechanism\r\n      - Disengaging or tooth breakage of wheel train\r\n        of the paper feed mechanism\r\n - Failed to read the PF motor encoder\r\n   2. Jumping of the PF timing belt\r\n   3. Contamination of the PF encoder scale\r\n   4. Skew or damage of the PF encoder FFC\r\n   5. Failure of the PF encoder sensor\r\n   6. Failure of the main board"

[PRN_000060]
MEANING="ASF PID driving time error"
DESCRIPTION="Malfunction or crash of the firmware"

[PRN_000061]
MEANING="ASF PID excess load error"
DESCRIPTION=" - The ASF motor stopped running in the middle of the operation\r\n   1. The ASF was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the ASF motor encoder\r\n   2. Disconnection or contamination of the ASF encoder scale\r\n   3. Disconnection, break, skew or damage of\r\n        the ASF motor cable/ASF encoder FFC\r\n   4. Failure of the ASF encoder sensor\r\n   5. Failure of the ASF motor (not completely broken)\r\n   6. Failure of the main board"

[PRN_000062]
MEANING="ASF PID excess speed error"
DESCRIPTION=" - Failed to read the ASF motor encoder\r\n   1. Contamination of the ASF encoder scale\r\n   2. Damage or skew of the ASF motor cable/encoder FFC\r\n   3. Failure of the ASF encoder sensor\r\n - Failure of the ASF motor driver\r\n   4. Failure of the main board"

[PRN_000063]
MEANING="ASF PID reverse error"
DESCRIPTION=" - Paper feed fails, stopped by obstacles\r\n   1. The ASF was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the ASF motor encoder\r\n   2. Contamination of the ASF encoder scale\r\n   3. Damage or skew of the ASF motor cable/encoder FFC\r\n   4. Failure of the ASF encoder sensor\r\n   5. Failure of the main board"

[PRN_000064]
MEANING="ASF PID lock error"
DESCRIPTION=" - The ASF motor did not run\r\n   1. The ASF was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the ASF motor encoder\r\n   2. Contamination of the ASF encoder scale\r\n   3. Disconnection, break, skew or damage of\r\n       the ASF motor cable/encoder FFC\r\n   4. Failure of the ASF encoder sensor\r\n   5. Failure of the ASF motor (the lead wire is broken\r\n       or the connector is disconnected)\r\n   6. Failure of the main board"

[PRN_000070]
MEANING="ASF load position driving time error"
DESCRIPTION="Malfunction or crash of the firmware"

[PRN_000071]
MEANING="ASF load position excess load error"
DESCRIPTION=" - The ASF motor stopped running in the middle of the operation\r\n   1. The ASF was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - ailed to read the ASF motor encoder\r\n   2. Contamination of the ASF encoder scale\r\n   3. Failure of the ASF encoder sensor\r\n   4. Failure of the ASF motor (not completely broken)\r\n   5. Failure of the main board"

[PRN_000072]
MEANING="ASF load position excess speed error"
DESCRIPTION=" - Failed to read the ASF motor encoder\r\n   1. Contamination of the ASF encoder scale\r\n   2. Damage or skew of the ASF motor cable/encoder FFC\r\n   3. Failure of the ASF encoder sensor\r\n - Failure of the ASF motor driver\r\n   4. Failure of the main board"

[PRN_000073]
MEANING="ASF load position reverse error"
DESCRIPTION=" - Paper feed fails, stopped by obstacles\r\n   1. The ASF was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the ASF motor encoder\r\n   1. Contamination of the ASF motor encoder scale\r\n   2. Damage or skew of the ASF motor cable/encoder FFC\r\n   3. Failure of the ASF motor encoder\r\n   4. Failure of the main board"

[PRN_000080]
MEANING="2ndASF PID driving time error"
DESCRIPTION="Malfunction or crash of the firmware"

[PRN_000081]
MEANING="2ndASF PID excess load error"
DESCRIPTION=" - The 2ndASF motor stopped running in the middle of the operation\r\n   1. The 2ndASF was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the 2ndASF motor encoder\r\n2. Disconnection or contamination of the 2ndASF encoder scale\r\n3. Disconnection, break, skew or damage\r\n    of the 2ndASF motor cable/encoder FFC\r\n4. Failure of the 2ndASF encoder sensor\r\n5. Failure of the 2ndASF motor (not completely broken)\r\n6. Failure of the main board"

[PRN_000082]
MEANING="2ndASF PID excess speed error"
DESCRIPTION=" - Failed to read the 2ndASF motor encoder\r\n   1. Contamination of the 2ndASF encoder scale\r\n   2. Damage or skew of the 2ndASF motor cable/encoder FFC\r\n   3. Failure of the 2ndASF encoder sensor\r\n - Failure of the 2ndASF motor driver\r\n   4. Failure of the main board"

[PRN_000083]
MEANING="2ndASF PID reverse error"
DESCRIPTION=" - Paper feed fails, stopped by obstacles\r\n   1. The 2ndASF was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the 2ndASF motor encoder\r\n   2. Contamination of the 2ndASF encoder scale\r\n   3. Damage or skew of the 2ndASF motor cable or encoder FFC\r\n   4. Failure of the 2ndASF encoder sensor\r\n   5. Failure of the main board"

[PRN_000084]
MEANING="2ndASF PID lock error"
DESCRIPTION=" - The 2ndASF motor did not run\r\n   1. The 2ndASF was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the 2ndASF motor encoder\r\n   2. Contamination of the 2ndASF encoder scale\r\n   3. Disconnection, break, skew or damage of\r\n       the 2ndASF motor cable/encoder FFC\r\n   4. Failure of the 2ndASF encoder sensor\r\n   5. Failure of the 2ndASF motor (the lead wire\r\n       is broken or the connector is disconnected)\r\n   6. Failure of the main board"

[PRN_000090]
MEANING="2ndASF load position driving time error"
DESCRIPTION="Malfunction or crash of the firmware"

[PRN_000091]
MEANING="2ndASF load position excess load errorエラ -"
DESCRIPTION=" - The 2ndASF motor stopped running in the middle of the operation\r\n   1. The 2ndASF was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the 2ndASF motor encoder\r\n   2. Contamination of the 2ndASF encoder scale\r\n   3. Failure of the 2ndASF encoder sensor\r\n   4. Failure of the 2ndASF motor (not completely broken)\r\n   5. Failure of the main board"

[PRN_000092]
MEANING="2ndASF load position excess speed error"
DESCRIPTION=" - Failed to read the 2ndASF motor encoder\r\n   1. Contamination of the 2ndASF encoder scale\r\n   2. Damage or skew of the 2ndASF motor cable or encoder FFC\r\n   3. Failure of the 2ndASF encoder sensor\r\n - Failure of the 2ndASF motor driver\r\n   4. Failure of the main board"

[PRN_000093]
MEANING="2ndASF load position reverse error"
DESCRIPTION=" - Paper feed fails, stopped by obstacles\r\n   1. The 2ndASF was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the 2ndASF motor encoder\r\n   1. Contamination of the 2ndASF motor encoder scale\r\n   2. Damage or skew of the 2ndASF motor cable or encoder FFC\r\n   3. Failure of the 2ndASF motor encoder\r\n   4. Failure of the main board"

[PRN_000100]
MEANING="IS PID driving time error"
DESCRIPTION="Malfunction or crash of the firmware"

[PRN_000101]
MEANING="IS PID excess load error"
DESCRIPTION=" - The I/S motor stopped running in the middle of the operation\r\n   1. The ink system was stopped by;\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the I/S encoder\r\n   2. Contamination of the I/S encoder scale\r\n   3. Failure of the I/S motor (not completely broken)\r\n   4. Failure of the main board"

[PRN_000102]
MEANING="IS PID excess speed error"
DESCRIPTION=" - Failed to read the I/S motor encoder\r\n   1. Contamination of the I/S encoder scale\r\n   2. Damage or skew of the I/S encoder FFC\r\n   3. Failure of the I/S encoder sensor\r\n - Failure of the I/S motor driver\r\n   4. Failure of the main board"

[PRN_000103]
MEANING="IS PID reverse error"
DESCRIPTION=" - Operation failure of the I/S motor, stopped by obstacles\r\n   1. The ink system was stopped by;\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the I/S encoder\r\n   2. Contamination of the I/S encoder scale\r\n   3. Damage or skew of the I/S motor cable/encoder FFC\r\n   4. Failure of the I/S encoder sensor\r\n   5. Failure of the main board"

[PRN_000104]
MEANING="IS PID lock error"
DESCRIPTION=" - The I/S motor did not run\r\n   1. The ink system was stopped by;\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the I/S encoder\r\n   2. Contamination of the I/S encoder scale\r\n   3. Break, skew or damage of the I/S motor cable/encoder FFC\r\n   4. Failure of the I/S encoder sensor\r\n   5. Failure of the I/S motor (the lead wire is broken or the\r\n       connector is disconnected)\r\n   6. Failure of the main board"

[PRN_000110]
MEANING="IS load position driving time error"
DESCRIPTION="Malfunction or crash of the firmware"

[PRN_000111]
MEANING="IS load position excess load error"
DESCRIPTION=" - The I/S motor stopped running in the middle of the operation\r\n   1. The ink system was stopped by;\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the I/S encoder\r\n   2. Contamination of the I/S encoder scale\r\n   3. Failure of the I/S motor (not completely broken)\r\n   4. Failure of the main board"

[PRN_000112]
MEANING="IS load position excess speed error"
DESCRIPTION=" - Failed to read the I/S encoder\r\n  1. Contamination of the I/S encoder scale\r\n  2. Damage or skew of the I/S encoder FFC\r\n  3. Failure of the I/S encoder sensor\r\n - Failure of the I/S motor driver\r\n  4. Failure of the main board"

[PRN_000113]
MEANING="IS load position reverse error"
DESCRIPTION=" - Operation failure of the I/S motor, stopped by obstacles\r\n  1. The ink system was stopped by;\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - ailed to read the I/S encoder\r\n  1. Contamination of the I/S motor encoder scale\r\n  2. Damage or skew of the I/S motor cable/encoder FFC\r\n  3. Failure of the I/S encoder sensor\r\n  4. Failure of the main board"

[PRN_000140]
MEANING="STK PID driving time error"
DESCRIPTION="Malfunction or crash of the firmware"

[PRN_000141]
MEANING="STK PID excess load error"
DESCRIPTION="  - The Stacker motor stopped running in the middle of the operation\r\n   1. The Stacker Open Unit was stopped by;\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the Stacker motor encoder\r\n   2. Contamination of the Stacker motor encoder scale\r\n   3. Failure of the Stacker motor (not completely broken)\r\n   4. Failure of the main board"

[PRN_000142]
MEANING="STK PID excess speed error"
DESCRIPTION=" - Failed to read the Stacker motor encoder\r\n   1. Contamination of the Stacker motor encoder scale\r\n   2. Damage or skew of the Stacker motor encoder FFC\r\n   3. Failure of the Stacker motor encoder sensor\r\n - Failure of the Stacker motor driver\r\n   4. Failure of the main board"

[PRN_000143]
MEANING="STK PID reverse error"
DESCRIPTION=" - Operation failure of the Stacker motor, stopped by obstacles\r\n   1. The Stacker open unit was stopped by;\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the Stacker motor encoder\r\n   2. Contamination of the Stacker motor encoder scale\r\n   3. Damage or skew of the Stacker motor cable/encoder FFC\r\n   4. Failure of the Stacker motor encoder sensor\r\n   5. Failure of the main board"

[PRN_000144]
MEANING="STK PID lock error"
DESCRIPTION=" - The Stacker motor did not run\r\n   1. The Stacker open unit was stopped by;\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the Stacker motor encoder\r\n   2. Contamination of the Stacker motor encoder scale\r\n   3. Break, skew or damage of the Stacker motor cable/encoder FFC\r\n   4. Failure of the Stacker motor encoder sensor\r\n   5. Failure of the Stacker motor (the lead wire is broken or the\r\n       connector is disconnected)\r\n   6. Failure of the main board"

[PRN_000150]
MEANING="STK load position driving time error"
DESCRIPTION="Malfunction or crash of the firmware"

[PRN_000151]
MEANING="STK load position excess load error"
DESCRIPTION=" - The Stacker motor stopped running in the middle of the operation\r\n   1. The Stacker open unit was stopped by;\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the Stacker motor encoder\r\n   2. Contamination of the Stacker motor encoder scale\r\n   3. Failure of the Stacker motor (not completely broken)\r\n   4. Failure of the main board"

[PRN_000152]
MEANING="STK load position excess speed error"
DESCRIPTION=" - Failed to read the Stacker motor encoder\r\n  1. Contamination of the Stacker motor encoder scale\r\n  2. Damage or skew of the Stacker motor encoder FFC\r\n  3. Failure of the Stacker motor encoder sensor\r\n - Failure of the Stacker motor driver\r\n  4. Failure of the main board"

[PRN_000153]
MEANING="STK load position reverse error"
DESCRIPTION=" - Operation failure of the Stacker motor, stopped by obstacles\r\n  1. The Stacker open unit was stopped by;\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - ailed to read the Stacker motor encoder\r\n  1. Contamination of the Stacker motor encoder scale\r\n  2. Damage or skew of the Stacker motor cable/encoder FFC\r\n  3. Failure of the Stacker motor encoder sensor\r\n  4. Failure of the main board"

[PRN_000680]
MEANING="RASF PID driving time error"
DESCRIPTION="Malfunction or crash of the firmware"

[PRN_000681]
MEANING="RASF PID excess load error"
DESCRIPTION=" - The RASF motor stopped running in the middle of the operation\r\n   1. The RASF unit was stopped by;\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the RASF encoder\r\n   2. Contamination of the RASF encoder scale\r\n   3. Failure of the RASF motor (not completely broken)\r\n   4. Failure of the main board"

[PRN_000682]
MEANING="RASF PID excess speed error"
DESCRIPTION=" - Failed to read the RASF motor encoder\r\n   1. Contamination of the RASF encoder scale\r\n   2. Damage or skew of the RASF encoder FFC\r\n   3. Failure of the RASF encoder sensor\r\n - Failure of the RASF motor driver\r\n   4. Failure of the main board"

[PRN_000683]
MEANING="RASF PID reverse error"
DESCRIPTION=" - Operation failure of the RASF motor, stopped by obstacles\r\n   1. The RASF unit was stopped by;\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the RASF encoder\r\n   2. Contamination of the RASF encoder scale\r\n   3. Damage or skew of the RASF motor cable/encoder FFC\r\n   4. Failure of the RASF encoder sensor\r\n   5. Failure of the main board"

[PRN_000684]
MEANING="RASF PID lock error"
DESCRIPTION=" - The RASF motor did not run\r\n   1. The RASF unit was stopped by;\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the RASF encoder\r\n   2. Contamination of the RASF encoder scale\r\n   3. Break, skew or damage of the RASF motor cable/encoder FFC\r\n   4. Failure of the RASF encoder sensor\r\n   5. Failure of the RASF motor (the lead wire is broken or the\r\n       connector is disconnected)\r\n   6. Failure of the main board"

[PRN_000690]
MEANING="RASF load position driving time error"
DESCRIPTION="Malfunction or crash of the firmware"

[PRN_000691]
MEANING="RASF load position excess load error"
DESCRIPTION=" - The RASF motor stopped running in the middle of the operation\r\n   1. The RASF unit was stopped by;\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read the RASF encoder\r\n   2. Contamination of the RASF encoder scale\r\n   3. Failure of the RASF motor (not completely broken)\r\n   4. Failure of the main board"

[PRN_000692]
MEANING="RASF load position excess speed error"
DESCRIPTION=" - Failed to read the RASF encoder\r\n  1. Contamination of the RASF encoder scale\r\n  2. Damage or skew of the RASF encoder FFC\r\n  3. Failure of the RASF encoder sensor\r\n - Failure of the RASF motor driver\r\n  4. Failure of the main board"

[PRN_000693]
MEANING="RASF load position reverse error"
DESCRIPTION=" - Operation failure of the RASF motor, stopped by obstacles\r\n  1. The RASF unit was stopped by;\r\n      - Overload of the mechanism\r\n      - Disengaging or breakage of the gears\r\n - ailed to read the RASF encoder\r\n  1. Contamination of the RASF motor encoder scale\r\n  2. Damage or skew of the RASF motor cable/encoder FFC\r\n  3. Failure of the RASF encoder sensor\r\n  4. Failure of the main board"

[PRN_000700]
MEANING="EJ2 PID driving time error"
DESCRIPTION="Malfunction or crash of the firmware"

[PRN_000701]
MEANING="EJ2 PID excess load error"
DESCRIPTION=" - The EJ2 motor stopped running in the middle of the operation\r\n   1. The EJ2 was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the paper feed mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read The EJ2 motor encoder\r\n   2. The timing belt become frayed or jumping\r\n   3. Contamination of The EJ2 encoder scale\r\n   4. Disconnection, break, skew or damage\r\n       of The EJ2 motor cable/encoder FFC\r\n   5. Failure of The EJ2 motor (not completely broken)\r\n   6. Failure of the main board"

[PRN_000702]
MEANING="EJ2 PID excess speed error"
DESCRIPTION=" - Failed to read The EJ2 motor encoder\r\n   1. Contamination of The EJ2 encoder scale\r\n   2. Skew or damage of The EJ2 encoder FFC\r\n   3. Failure of The EJ2 encoder sensor\r\n - Failure of The EJ2 motor driver\r\n   4. Failure of the main board"

[PRN_000703]
MEANING="EJ2 PID reverse error"
DESCRIPTION=" - Paper feed fails, stopped by obstacles\r\n   1. Paper feed was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the paper feed mechanism\r\n      - Disengaging or tooth breakage of wheel train\r\n        of the paper feed mechanism\r\n - Failed to read The EJ2 motor encoder\r\n   2. Jumping of The EJ2 timing belt\r\n   3. Contamination of The EJ2 encoder scale\r\n   4. Skew or damage of The EJ2 encoder FFC\r\n   5. Failure of The EJ2 encoder sensor\r\n   6. Failure of the main board"

[PRN_000704]
MEANING="EJ2 PID lock error"
DESCRIPTION=" - The EJ2 motor did not run or obstacles exist in the paper path\r\n   1. Overload of the paper feed mechanism\r\n   2. The EJ2 timing belt become frayed, jumping,\r\n        or the wheel train of paper feed mechanism\r\n        is disengaged or its tooth is broken\r\n - Failed to read The EJ2 motor encoder\r\n   3. Contamination of The EJ2 encoder scale\r\n   4. Disconnection, break, skew or damage of The EJ2 encoder FFC\r\n   5. Failure of The EJ2 encoder sensor\r\n   6. Failure of The EJ2 motor (the lead wire is broken\r\n       or the connector is disconnected)\r\n   7. Failure of the main board"

[PRN_000710]
MEANING="EJ2 load position driving time error"
DESCRIPTION="Malfunction or crash of the firmware"

[PRN_000711]
MEANING="EJ2 load position excess load error"
DESCRIPTION=" - The EJ2 motor stopped running in the middle of the operation\r\n   1. The EJ2 was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the paper feed mechanism\r\n      - Disengaging or breakage of the gears\r\n - Failed to read The EJ2 motor encoder\r\n   2. Jumping of the timing belt\r\n   3. Contamination of The EJ2 encoder scale\r\n   4. Failure of The EJ2 motor (not completely broken)\r\n   5. Failure of the main board"

[PRN_000712]
MEANING="EJ2 load position excess speed error"
DESCRIPTION=" - Failed to read The EJ2 motor encoder\r\n   1. Contamination of The EJ2 encoder scale\r\n   2. Skew or damage of The EJ2 encoder FFC\r\n   3. Failure of The EJ2 encoder sensor\r\n - Failure of The EJ2 motor driver\r\n   4. Failure of the main board"

[PRN_000713]
MEANING="EJ2 load position reverse error"
DESCRIPTION=" - Paper feed fails, stopped by obstacles\r\n   1. Paper feed was stopped by;\r\n      - Obstacles such as jammed paper\r\n      - Overload of the paper feed mechanism\r\n      - Disengaging or tooth breakage of wheel train\r\n        of the paper feed mechanism\r\n - Failed to read The EJ2 motor encoder\r\n   2. Jumping of The EJ2 timing belt\r\n   3. Contamination of The EJ2 encoder scale\r\n   4. Skew or damage of The EJ2 encoder FFC\r\n   5. Failure of The EJ2 encoder sensor\r\n   6. Failure of the main board"

[PRN_030004]
MEANING="emergency error of cover opened"
DESCRIPTION="If rear unit is removed durling motor moving,the printer stops motor at an emergency to occur error in order to ensure the safety\r\n1.Failed to　install rear unit\r\n2.Failure of　installing sensor of rear unit"

[PRN_031001]
MEANING="HeadHot detect error (pre printing)"
DESCRIPTION=" - Disconnection, break, skew or damage of the head FFC\r\n - Overheat of the printhead\r\n   1. Failure of the printhead\r\n   2. Failure of the main board\r\n      - Occurs in -between print passes\r\n         (after printing one pass and before printing the next pass)"

[PRN_031002]
MEANING="HeadHot detect error (after flushing)"
DESCRIPTION=" - Disconnection, break, skew or damage of the head FFC\r\n - Overheat of the printhead\r\n   1. Failure of the printhead\r\n   2. Failure of the main board\r\n      - Occurs every after ink flushing operation\r\n          (Flushing before starting printing, flushing\r\n           after manual cleaning and etc.)"

[PRN_031003]
MEANING="Transistor temperature error"
DESCRIPTION=" - Failure of the main board\r\n- Occurs after receiving a print job and starting printing"

[PRN_031004]
MEANING="Head temperature error"
DESCRIPTION=" - Disconnection, break, skew or damage of the head FFC\r\n     - Occurs after receiving a print job and starting printing\r\nFailure of the thermistor inside the printhead.\r\n        Temperature around the printhead is out of the range from  -20 to 80 degrees C."

[PRN_031006]
MEANING="Blowout of a fuse error (Head)"
DESCRIPTION=" - Failure of the power source for the\r\nprinthead\r\n  1. Failure of the circuit Disconnection, break, skew, or\r\ndamage of the head FFC\r\n  2. Blowout of fuse on the main board Failure of the printhead\r\n     - Occurs at power -on, when replacing the ink cartridge, inbetween print passes, and after flushing operation"

[PRN_031008]
MEANING="VBS overvoltage error"
DESCRIPTION="1. Head FFC failure (skew, foreign object attached)\r\n2. Failure of the head\r\n3. Failure of the main board\r\n(Occurrence frequency based on past record is 1. > 2. > 3.)"

[PRN_031011]
MEANING="HCS error"
DESCRIPTION=" - Error in the diverted head measure\r\n - Does not occurs at ordinary using\r\n - Occurs at failure of the head (be unlikely but not impossible)"

[PRN_033001]
MEANING="Blowout of a fuse error (CRCM)"
DESCRIPTION=" - Failure of the main board\r\n     - Occurs at power -on, and during operation\r\n         for replacing the ink cartridge"

[PRN_033003]
MEANING="Other Ink device error"
DESCRIPTION=" - Error in the printer settings\r\n - Failure of the main board\r\n     - Occurs at power -on"

[PRN_033004]
MEANING="Other Ink device error"
DESCRIPTION=""

[PRN_033005]
MEANING="Other Ink device error"
DESCRIPTION=""

[PRN_033006]
MEANING="CRCM access error（Hard factor）"
DESCRIPTION=" - Disconnection, break, skew or damage of the CRCM FFC\r\n - Failure of the CSIC terminal/CR contact module\r\n - Failure of the main board"

[PRN_033007]
MEANING="CRCM access error（Hard factor）"
DESCRIPTION=""

[PRN_033008]
MEANING="CRCMアクセスエラー（ファーム要因）
※工程のみ発生し、本エラーコードは表示されることはない"
DESCRIPTION="※工程のみ発生し、本エラーコードは表示されることはない"

[PRN_033010]
MEANING="CSIC access error（Hard factor）"
DESCRIPTION=" - Disconnection, break, skew or damage of the CRCM FFC\r\n - Failure of the CSIC terminal/CR contact module\r\n - Failure of the main board (mismatch of the printer settings that cannot be changed when repairing the printer)\r\n     - Occurs at power -on"

[PRN_033501]
MEANING="ILS environmental error"
DESCRIPTION="The PIS sensor received unexpected amount of light"

[PRN_033502]
MEANING="ILS continuous reflected light error"
DESCRIPTION=" - The PIS sensor received unexpected amount of reflected light from the jig I/C\r\n - Anti -reflection film of the I/C has been removed"

[PRN_033503]
MEANING="ILS no reflected light error"
DESCRIPTION=" - Electric voltage for the PIS sensor is\r\ninsufficient\r\n   - Break of the FFC\r\n   - The PIS sensor has deteriorated\r\n   - Reflected light from the I/C is insufficient\r\n     - At power -on, during replacing I/C"

[PRN_033504]
MEANING="ILS shift length error"
DESCRIPTION="Positioning of the I/C and the PIS sensor is inaccurate."

[PRN_033505]
MEANING="ILS Empty Jig error"
DESCRIPTION="Light from Empty jig I/C is insufficient"

[PRN_033506]
MEANING="Excessive Light error"
DESCRIPTION="Light from Full jig I/C is too much"

[PRN_033507]
MEANING="Insufficient Light error"
DESCRIPTION=" - Electric voltage for the PIS sensor is insufficient\r\n   - Break of the FFC\r\n   - The PIS sensor has deteriorated\r\n   - Reflected light from the I/C is insufficient\r\n     - At power -on, during replacing I/C, during switching APG"

[PRN_034001]
MEANING="Home position error
※パネル表示は紙ジャムエラーでユーザーは気付かないが、エラー履歴は残る"
DESCRIPTION="This error code is not displayed but the\r\nerror history is saved.\r\n - The carriage does not move\r\n  1. Overload of the carriage drive mechanism (paper jam, foreign object)\r\n  2. Failure of the ink system\r\n  3. Failure of the CR motor\r\n  4. Failure of the main board"

[PRN_034019]
MEANING="APG error"
DESCRIPTION="Failed to move PG swiching structure\r\n - When CR push in gear of PG swiching structure,CR can't push in gear due to have a bad bite\r\n - Failure of PG swiching structure"

[PRN_034500]
MEANING="Ink cartridge replacement timing contact detection error"
DESCRIPTION="Because the I/C is not securely installed, it comes in contact with the housing."

[PRN_060001]
MEANING="Factor error other than printer device
※ダミーコードであり、本エラーコードは表示されることはない"
DESCRIPTION=" -"

[PRN_060002]
MEANING="Driver mismatch error"
DESCRIPTION=" - Non -supported printer driver\r\n - Mismatch between custom printer driver and custom printer."

[PRN_060003]
MEANING="PCD verify error (by command)
※工程のみ発生し、本エラーコードは表示されることはない"
DESCRIPTION=" -"

[SYS_202620]
MEANING="Wi -Fi Board failure"
DESCRIPTION="Failure or disconnection of the wireless network board"

[SYS_205102]
MEANING="Card Slot Board failure"
DESCRIPTION="カード基板故障・非接続"

